Maximal volumetric flow (mm^3/sec)
Volumetric flow is calculate as follows:

(layer thickness) x (nozzle diameter) x (printing speed)

IceSL caps the printing speed as to not exceed this value.
Set it to zero (0) if no limit is desired.