Maximum curving angle (degrees)
Sets the angle beyond which curving is strictly
forbidden. This setting should be used to avoid
collision of the nozzle with the print when the
slices are steeply curved.