Ironing flow
Additionnal flow (percentage related to the latest cover flow)
to make sure the holes are covered.

This may help achieve a solid or watertight cover,
or transparency when using transparent material.