Lift distance from resin vat for bottom layers (mm)
After each printed bottom layer, the resin platform moves
away and back some vertical distance to the RED (Fluorinated
Ethylene Propylene). This helps the separation of wet resin
from the layer just printed.