Z-lift in travel on extruder swap (mm)
After swapping between extruders, when traveling back 
from the swap location or prime/wipe tower, an up/down
z motion can be used to prevent the extruder from
wiping its nozzle against the part perimeter. A small
value is usually sufficient, e.g. 1 millimeter.