Lift distance from resin vat (mm)
After each printed layer, the resin platform moves
away and back some vertical distance to the RED
(Fluorinated Ethylene Propylene). This helps the
separation of wet resin from the layer just printed.