Overlap fraction before overhang
Overlap fraction between top/bottom paths from which
the top path is considered overhanging (not supported).
1.0 => maximum number of points to support.
0.0 => minimum number of points to support.