Target temperature when idle (C)
This parameter is needed when using active temperature
control. This is the target temperature of the idle extruder.
Select the highest value that does not produce oozing
and ensures the material will not degrade in the nozzle.