Distance between brim and print (mm)
Distance in millimeters (mm) between the surrounding
brim and the object to be printed. Use 0.0 to use the
brim as a skirt attached to the base layer and stabilize
the print.