Compute fan speed w.r.t. overhang angle
Automatically compute fan speed over the geometry according
to an overhang angle. The closer the geometry's inclination
(i.e., angle w.r.t. Z axis) is to a user-defined overhang
angle, the faster the fan is set (i.e., material cools down
quicker). The range of fan speeds are also user-defined.