Force backtrack on first layer
Enable backtrack on all printing paths for the first layer.
This will force the printer to make a "dry move"
back to the start of a deposition path to ensure
the first layer is correctly deposited.

This setting can induce a significant increase on
print time for the first layer.

This is particularly indicated when using Polyfoams
or any infill with many small cells.