Tower size along Y (mm)
Size of the tower along Y direction. Increase if the 
extruder is not properly primed (holes when the 
extruder resumes printing after a swap), or if the 
tower is not stable enough when it becomes tall.