Avoid traveling within top (visible) covers
When enabled, the travel optimizer will avoid 
traveling within the top (visible) covers. 
Enable if the extruder leaves a visible mark on 
flat top surfaces. Leave disabled for faster 
processing if the print has few top flat surfaces,
or if aesthetics are not a concern.