Min. space between supported points (mm)
Minimal spacing (in millimeters) between the contact
points covering overhanging surfaces.
Lowering this value makes the support denser,  
increasing the quality of bottom surfaces but 
making the support more difficult to remove.